Summary of Changes

Effective Monday, March 20, 2107, CenturyLink will implement Version 54 of the Access Services Ordering Guidelines within its Pre-Order and Ordering Interface systems.

During the release implementation, EASE VFO (Virtual Front Office) and UOM (Unified Ordering Model) will be unavailable for processing transactions from 5:00 PM ET on Friday, March 17th, 2016 until 7:00 AM ET on Monday, March 20, 2017.

CenturyLink will modify product based edits including, but not limited to, the following:

*Please NOTE: A complete list of EASE custom edits can be viewed by clicking on the web-link for ASR CenturyLink Custom Business Rules available from the EASE Homepage in the Guide (ASR) TAB.*

| **Action** | **ASR Form** | **Field** | **Business Rule / WEBCALL / EDIT** |
| --- | --- | --- | --- |
| Add | ASR | SITE CON | SITE CON - Site Contact Identifies the site contact name for access when the customer utilizes a Carrier Hotel as the primary location. NOTE 1: This field should be used in conjunction with the TEL NO (SITE CON) and SITE EMAIL fields on this form. NOTE 2: When the SALI Form is present, this field is used to provide supplemental site information in addition to the LCON field. USAGE: This field is optional. |
| Add | ASR | TEL NO  (SITE CON) | TEL NO (SITE CON) - Site Contact Telephone Number Identifies the telephone number of the Site Contact. USAGE: This field is conditional. NOTE 1: Required when the SITE CON field is populated, otherwise prohibited.  DATA CHARACTERISTICS: 17 numeric characters (excluding 3 preprinted hyphens) EXAMPLES: 2 0 1 - 9 8 1 - 3 5 8 7 - 3 2 5 7 |
| Add | ASR | SITE EMAIL | SITE EMAIL - Site Contact Electronic Mail Address Identifies the electronic mail address of the Site Contact. USAGE: This field is conditional. NOTE 1: Optional when the SITE CON field is populated, otherwise prohibited. |
| Change | ASR | REQTYP | Valid entries Step 1 – G = Access Service Request (ASR) follow up to verbal Customer |
| Change | ASR | REQTYP | Valid entries Step 3A – Firm Order – (Service Request Inquiry Sent, (Same PON) |
| Change | ASR | REQTYP | Valid entries Step 3A – J = Access Service Request (ASR) follow up to verbal Customer |
| Change | ASR | REQTYP | Valid entries Step 3B – Firm Order – (Service Request Inquiry Not Sent, Direct to Firm Order) |
| Change | ASR | REQTYP | Valid entries Step 3B – J = Access Service Request (ASR) follow up to verbal |
| Change | ASR | IWBAN | Addition of value "H": NOTE 1: Required when the GETO field on the service specific form is “A”, “E”, “H”, “S”, “T”, “U”, “V”, “W”, “Y”, or “Z”. |
| Change | TRANSPORT | GETO | Addition of value: H = Provide entrance facility from curb to Minimum Point Of Entry (MPOE) and inside wiring and bill the customer |
| Change | TRANSPORT | GETO | Addition of values H to valid entries NOTE 4: When the valid entry is other than “H”, “F”, “N”, “S”, “U”, or “W”, the General Exchange Tariff Options Contact Name (GCON) field must be populated. |
| Change | TRANSPORT | GBTN | Addition of values F & H to usage Note 1 NOTE 1: Prohibited when the GETO field is “A”, “E”, “F”, “H”, “S”, “T”, “U”, “V”, “W”, “Y”, “Z” or not populated, otherwise optional. |
| Change | MSL | GETO | Addition of values to valid entries: F = Provide entrance facility from curb to Minimum Point Of Entry (MPOE) and bill the customer. H = Provide entrance facility from curb to Minimum Point Of Entry (MPOE) and inside wiring and bill the customer |
| Change | MSL | GETO | Addition of values to valid entries: Note 4: When the valid entry is other than “F”, “H”, “N”, “S”, “U” or “W”, the GCON field must be populated. |
| Change | MSL | GBTN | Addition of values to usage: NOTE 1: Prohibited when the GETO field is “A”, “E”, “F”, “H”, “S”, “T”, “U”, “V”, “W”, “X”, “Y”, “Z” or not populated, otherwise optional. |
| Change | SES | GETO | Addition of value to valid entries: H = Provide entrance facility from curb to Minimum Point Of Entry (MPOE) and inside wiring and bill the customer |
| Change | SES | GETO | Addition of values to valid entries: NOTE 4: When the valid entry is other than “F”, “H”, “N”, “S”, “U” or “W”, the GCON field must be populated. |
| Change | SES | GBTN | Addition of values to usage: NOTE 1: Prohibited when the GETO field is “A”, “E”, “F”, “H”, “S”, “T”, “U”, “V”, “W”, “Y”, “Z” or not populated, otherwise optional. |
| Change | CN/R | General | Updated verbage: This form is intended to streamline the process between customers and providers to resolve discrepancies on the ASR. It is not intended to replace existing error notification procedures; however, it may be used to augment them. The C/NR may occur anytime during the order process and may result in multiple C/NRs being issued. Use of the C/NR Form does not replace existing business processes for confirmation. The form can be used to provide the following information to the customer: |
| Change | EUSA | GETO(PRILOC) | Addition of value to valid entries: H = Provide entrance facility from curb to Minimum Point Of Entry (MPOE) and inside wiring and bill the customer |
| Change | EUSA | GETO(PRILOC) | Addition of values to valid entries: NOTE 4: When the valid entry is other than “F”, “H”, “N”, “S”, “U” or “W”, the GCON (PRILOC) field must be populated. |
| Change | EUSA | GBTN(PRILOC) | Addition of values to usage: NOTE 1: Prohibited when the GETO (PRILOC) field is “A”, “E”, “F”, “H”, “S”, “T”, “U”, “V”, “W”, “Y”, “Z” or not populated, otherwise optional. |
| Change | EUSA | GETO(SECLOC) | Addition of value to valid entries: H = Provide entrance facility from curb to Minimum Point Of Entry (MPOE) and inside wiring and bill the customer |
| Change | EUSA | GETO(SECLOC) | Addition of values to valid entries: NOTE 4: When the valid entry is other than “F”, “H”, “N”, “S”, “U” or “W”, the GCON (SECLOC) field must be populated. |
| Change | EUSA | GETO(SECLOC) | Addition of values to usage: NOTE 1: Prohibited when the GETO (SECLOC) field is “A”, “E”, “F”, “H”, “S”, “T”, “U”, “V”, “W”, “Y”, “Z” or not populated, otherwise optional. |
| Change | SALI | JK NUM | Updated definition NOTE 1: When the jack identification is unknown, enter 99 in this field. Required when the JS field is “E” or “N”. |
| Change | EVC | OTC | Updated usage NOTE 1: Required when the associated EVCMPIDASC-EC field on the ASR form is populated, otherwise prohibited. |
| Remove | ECI | CHPD | Field removed |
| Remove | ECI | PEND ORD | Field removed |
| Remove | ECI | SM | Field removed |
| Remove | ECI | SM2 | Field removed |
| Remove | ECI | SM3 | Field removed |
| Remove | ECI | SM4 | Field removed |
| Remove | ECI | SM5 | Field removed |
| Remove | ECI | SM6 | Field removed |
| Remove | ECI | SM7 | Field removed |
| Remove | ECI | QOPT | Field removed |
| Remove | ECI | PCT | Field removed |
| Remove | ECI | EASPEED | Field removed |
| Remove | ECI | EA TYPE | Field removed |
| Remove | ECI | CONFIG REMARKS | Field removed |
| Remove | ECI | ACPON | Field removed |
| Remove | ECI | ACAT | Field removed |
| Remove | ECI | TNT | Field removed |
| Remove | ECI | ACCESSID | Field removed |
| Remove | ECI | ACCESSORD | Field removed |
| Remove | ECI | PORTID | Field removed |
| Remove | ECI | PORTORD | Field removed |
| Remove | ECI | VCCID | Field removed |
| Remove | ECI | VCORD | Field removed |
| Remove | ECI | SOPTCON | Field removed |
| Remove | ECI | SUBNET MASK | Field removed |
| Remove | ECI | TRM | Field removed |
| Remove | ECI | VPN NM | Field removed |
| Remove | ECI | OPT CON | Field removed |
| Remove | ECI | IPAI | Field removed |
| Remove | ECI | IP ADDRESS | Field removed |
| Remove | ECI | ICID | Field removed |
| Remove | ECI | EXDI | Field removed |
| Remove | ECI | EGRESS | Field removed |
| Remove | ECI | EAID | Field removed |
| Remove | ECI | ASN | Field removed |