**TOS (Type of Service) Codes to be used in EASE**

**NOTE:** 4 Character TOS codes are required in EASE.

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Products | 1st Character | 2nd Character | 3rd Character | 4th Character |
| Bulk (GUI Only) | N/A | N/A | N/A | N/A |
| Enhanced Extended Loop (EEL) | 1 or 3; an EEL for a residence service must be ordered using TOS=1 | - | - | - |
| Directory Listings & Assistance | 1 or 2 | - | - | - |
| Line Sharing/Shared Loop  TOS for Loop Splitting = 1N, 2N, 3N | 1, 2 or 3; TOS=1 or 3 will be treated as business service | * R (Data/ Voice Line Sharing)  or * S  (Data/ Voice Line Splitting) Or * N (Data/Voice Loop  Splitting) | - | - |
| Local Number Portability (LNP) | 1, 2 or 3 | - | - | - |
| Resale - Centrex 21 | 1 or 3; TOS=1 or 3 will be treated as business service | E (Centrex) | * F (Flat) | - |
| Resale - Centrex Plus & Centron | 1, 2 or 3; TOS=1 or 3 will be treated as business service; | E (Centrex) | * M (Measured) or * F (Flat) | - |
| Resale - DID Trunks | 1 or 3 | J (PBX Trunk) | * M (Measured) or * F (Flat) | F (FXS)  Or  - |
| Resale - ISDN BRI | 1, 2 or 3; TOS=1 or 3 will be treated as business service | H (ISDN BRI) | * M (Measured) or * F (Flat) | F (FXS) or  - |
| Resale - ISDN PRI Facility | 1 or 3; TOS=1 or 3 will be treated as business service | K (PRI ISDN) | F (Flat) | F (FXS)  or  - |
| Resale - ISDN PRI Trunks | 1 or 3; TOS=1 or 3 will be treated as business service | K (PRI ISDN) | F (Flat) | F (FXS) or  - |
| Resale - PAL | 4; 4 will be treated as a business service | * C = Basic Coin * T = Smart Coin | - | - |
| Resale - PBX Trunk Service | 1, 2 or 3; TOS=1 or 3 will be treated as business service | J (PBX Trunk) | - | - |
| Resale - PBX Trunk Service – Designed | 1 or 3 | J (PBX Trunk) | * M (Measured) or * F (Flat) | F (FXS) or  - |
| Resale – POTS  . | 1, 2 or 3; TOS=1 or 3 will be treated as business service | * A (Multi-Line POTS)  or * B (Single Line POTS) | - | - |
| Resale – Private Line Transport (PLT) - Non-switched | 1 or 3 | - | - | - |
| Unbundled Distribution Loop (UDL) | 1, 2 or 3; TOS=1 or 3 will be treated as business service | P (Sub Loop Distribution) | - | - |
| Unbundled Distribution Loop (UDL)/Local Number Portability (LNP) | 1, 2 or 3; TOS=1 or 3 will be treated as business service | P (Sub Loop Distribution) | - | - |
| Unbundled Feeder Loop (UFL) | 1, 2 or 3; TOS=1 or 3 will be treated as business service | O (Sub Loop Feeder) | - | - |
| Unbundled Local Loop | 1, 2 or 3; TOS=1, 2 or 3 will be treated the same | - | - | - |
| Unbundled Local Loop Split | 1, 2 or 3; TOS=1, 2 or 3 will be treated the same | N | - | - |
| Unbundled Local Loop Split/Local Number Portability (LNP) | 1, 2 or 3; TOS=1, 2 or 3 will be treated the same | N | - | - |
| Unbundled Local Loop/Local Number Portability (LNP) | 1, 2 or 3; TOS=1, 2 or 3 will be treated the same | - | - | - |
| UNE-P – Centrex 21 | 1 or 3 | E (Centrex) | F (Flat) | - |
| UNE-P - Centrex 21 Split | 1 or 3 | E (Centrex) | F (Flat) | - |
| UNE-P – Centrex Plus and UNE-P – Centron | 1, 2 or 3; TOS=1 or 3 will be treated as business service; TOS=2 will be treated as residence service | E (Centrex) | F (Flat) | - |
| UNE-P - ISDN BRI | 1, 2 or 3; TOS=1 or 3 will be treated as business service | H (ISDN BRI) | M (Measured) or  F (Flat) | F (FXS)  or  - |
| UNE-P - PBX Trunks | 1 or 3 | J (PBX Trunk) | M (Measured) or  F (Flat) | F (FXS)  Or  - |
| UNE-P - PBX Trunks Split | 1 or 3 | J (PBX Trunk) | M (Measured) or  F (Flat) | F (FXS)  Or  - |
| UNE-P - PBX/DID Trunks | 1 or 3 | J (PBX Trunk) | M (Measured) or  F (Flat) | F (FXS)  Or  - |
| UNE-P POTS | 1, 2 or 3; TOS=1 or 3 will be treated as business service | * A (Multi-Line POTS) or * B (Single Line POTS) | M (Measured) | - |
| UNE-P POTS Split | 1, 2 or 3; TOS=1 or 3 will be treated as business service | * S = Data/Voice Line Splitting | M (Measured) | - |