IMA to EASE Differences

[Overview 2](#_Toc40421459)

[Introduction 2](#_Toc40421460)

[Pre-Order 3](#_Toc40421461)

[Address Validation 3](#_Toc40421462)

[Raw Loop Data 3](#_Toc40421463)

[Appointment Scheduler 3](#_Toc40421464)

[Order 4](#_Toc40421465)

[Local Service Request (LSR) 4](#_Toc40421466)

[End User (EU) 8](#_Toc40421467)

[Loop Service Form (LS) 11](#_Toc40421468)

[Number Portability (NP) 12](#_Toc40421469)

[Loop Service with Number Portability (LSNP) 13](#_Toc40421470)

[Resale Service (RS) 14](#_Toc40421471)

[Resale Private Line (RPL) 15](#_Toc40421472)

[Centrex Resale Services (CRS) 20](#_Toc40421473)

[DID/DOD/PBX Service (DDPS) – Compared to IMA Resale form (RS) 23](#_Toc40421474)

[DID/DOD/PBX Service (DDPS) – Compared to IMA DID Resale form (DRS) 26](#_Toc40421475)

[Hunt Group Information (HGI) 27](#_Toc40421476)

[ISDN BRI/PRI Service (IS) – Compared to IMA Resale form (RS) 28](#_Toc40421477)

[Directory Listing (DL) 29](#_Toc40421478)

[Miscellaneous 31](#_Toc40421479)

IMA to EASE Differences

# Overview

|  |  |
| --- | --- |
| Introduction | The intent of this document is to call out variances on where data was available in the IMA application and where it will be available in the EASE application. |

|  |  |
| --- | --- |
| Pre-Order | Below is the listing of differences between IMA and EASE for the PreOrder functions. |

| **Function** | **IMA Field** | **EASE Field** | **Modification** |
| --- | --- | --- | --- |
| Address Validation | | | |
| By TN | WTN | WTN | Add dashes to TN |
| Raw Loop Data | | | |
| RLD |  | RLD BY TN | Add LSO data. No dashes in TN |
| RLD | PAIR GAIN TYPE | TRMED | Data from PAIR GAIN TYPE field will now be provided in TRMED |
| RLD | LCT | LCQ | Data from LCT field will now be provided in LCQ |
| RLD | CABLE NAME | CA | Data from CABLE NAME field will now be provided in CA |
| RLD | PAIR GAIN TYPE | TRMED | Data from PAIR GAIN TYPE field will now be provided in TRMED |
| RLD | PAIR NUMBER | CHAN\_PAIR | Data from PAIR NUMBER field will now be provided in CHAN\_PAIR |
| Appointment Scheduler | | | |
|  | Enter Other Work Required USOC | FEAT\_PP | Enter USOCs in FEAT\_PP field |

|  |  |
| --- | --- |
| Order | Below is a summary of differences between ordering in IMA and EASE ordering forms. |

| **Function** | **IMA** | **EASE** | **Modification** |
| --- | --- | --- | --- |
| Local Service Request (LSR) | | | |
| 3.2 Administrative Section |  |  |  |
|  | LSRRO | N/A | Will not be needed |
|  | DLEC CCNA | OCCNA | Use OCCNA |
|  | PG\_of\_ | PG\_of\_ | BRMS rule to only allow 4 characters |
|  | TEST | SPEC | Use one of the values listed below  A = Performance Testing  B = Cooperative Testing  N = No Testing  I = Cooperative Testing |
| REQTYP | EB | NB | Resale Designed Trunks and set P field to A |
| REQTYP | EB | NB | Resale PBX POTS Trunks and set P field to A |
| REQTYP | MB | NB | CLSP PBX DID and set P field to C |
| REQTYP | MB | NB | CLSP PBX Designed Trunks and set P field to C |
| REQTYP | MB | KB | Enhanced Extended Loop (EEL) and Loop Mux Combo (LMC) and enter LOOPEEL in SPEC field on LSR form |
| REQTYP | SB | MB | CLSP POTS Split |
| REQTYP | SB | MB | CLSP Centrex 21 Split |
| REQTYP | SB | NB | CLSP PBX Split |
| REQTYP | UB | AB | Unbundled Loop Split |
| REQTYP | DB | BB | Loop with Number Port Split |
| REQTYP | EB | QB | Resale PRI ISDN Trunk and set LSR P field to A |
| REQTYP | KB | KB | Resale PRI ISDN Facility |
| REQTYP | EB | QB | Resale ISDN BRI and set LSR P field to A |
| REQTYP | MB | QB | CLSP ISDN BRI and set LSR P field to C |
| REQTYP | HB | JB | HB (Listings Only) will use the alpha numeric RSID.  If the intent is for FBDL listings then use the all alpha character RSID. BRMS rule to only allow ACT = C when alpha numeric RSID value is used |
|  | NA | P | ISDN BRI and PBX products:  A = Resale  C = Combined loop and unbundled local switching (port) or CLSP |
| ACT | Z | V | Scenarios where ACT = Z was used, use ACT = V and EU form, ELT field set to A |
| ACT | Y | S | Resale POTS and CLSP POTS use ACT of S and LNA of S to Deny |
| ACT | B | B | Resale POTS and CLSP POTS use ACT of B and LNA of B to Restore from Deny |
| ACT | L | L | Resale POTS and CLSP POTS use ACT of L and LNA of B to Restore from Seasonal Service |
|  | RSTTYP | N/A | Discontinue use of RSTTYP field as RS form LNA field data will be used |
|  | CIP | N/A | Will not be utilized |
|  | CSO1 | N/A | Will not be utilized |
|  | CSO2 | N/A | Will not be utilized |
|  | PMI | MI | On ACT of T and a partial move, enter A or B in MI field |
|  | MI | MI | Legacy Qwest EASE LSRs won’t require the OCC field to be used in conjunction with the MI field |
|  | SCA | Conditioning Options | For Unbundled Loop and Unbundled Distribution Loop Non-Loaded or ADSL loop products: Use Conditioning Options field for values Y, 1, 2 or 3 |
|  | SPEC | SPEC | EEL/LMC LSRs will need the data of EEL in SPEC field |
|  | LSP AUTH NAME | LSP AUTH NAME | BRMS rule to only allow 15 characters |
|  | NPDI | NPDI | When porting a VOIP TN, use value of A. Previous IMA value was V |
| 3.2 Bill Section |  |  |  |
|  | BAN1 | BAN1 | Data returned on FOC will be formatted without dashes |
|  | BAN2 | BAN2 | Data returned on FOC will be formatted without dashes |
|  | N/A | NRI | Set to Y for Manual Handling LSR |
|  | ZIP | ZIP | BRMS rule to only allow 5 characters |
|  | TEL NO | TEL NO | 2Q19 allows 14 characters and IMA allowed 17 characters |
| 3.4 Contact Section |  |  |  |
|  | INIT | INIT | BRMS rule to only allow 15 characters |
|  | TEL NO | TEL NO | 2Q19 allows 14 characters and IMA allowed 17 characters (applies to all TEL NO fields in Contact section) |
|  | FAX NO | FAX NO | 2Q19 allows 10 characters and IMA allowed 12 characters (applies to all FAX NO fields in Contact section) |
|  | ZIP | ZIP | BRMS rule to only allow 5 characters |
| Remarks Section |  |  |  |
|  | REMARKS1 | REMARKS1 | 2Q19 allows 250 characters and IMA allowed 255 characters |
|  | REMARKS2 | REMARKS2 | 2Q19 allows 250 characters and IMA allowed 255 characters |
|  | MANUAL IND | NRI | Set NRI equal to Y |
|  | PENDING ORDER | N/A | Will not be utilized |
|  | PIC | N/A | This functionality will be addressed as a future release |
|  | LPIC | N/A | This functionality will be addressed as a future release |
| End User (EU) | | | |
| 3.2 Location and Access Section |  |  |  |
|  | AHN | AFT | When AHN is necessary populate AFT with C (Provider assigned house number) and provide AHN numeric data in SANO field |
|  | SASN | SASN | BRMS rule to only allow 50 characters |
|  | LD1 | LD1 | This field is designated for address unit: APT = Apartment LOT = Lot RM = Room SLIP = Slip SUIT = Suite UNIT = Unit Note: This is the format to be used on all forms for this field. |
|  | LD2 | LD2 | This field is designated for address elevation:  FLR – Floor  Note: This is the format to be used on all forms for this field. |
|  | LD3 | LD3 | This field is designated for address structure:  BLDG = Building  PIER = Pier  WNG = Wing  Note: This is the format to be used on all forms for this field. |
|  | AAI | AAI | 2Q19 field length 60 characters and IMA was 100 characters |
|  | CALA | N/A | Use Zip field |
|  | ACC | ACC | 2Q19 field length 45 characters and IMA was 255 characters |
|  | WSOP TEL NO | N/A | Enter WSOP TN in remarks |
|  | ELT | ELT | BRMS rule will not allow value of C |
|  | Use Service Address | SHAI | SHAI – Shipping Address Indicator - Indicates if the shipping address should be used in lieu of the service address. Values: Y or N |
|  | SHAPR | SHAPR | BRMS rule will only allow 5 characters |
|  | SHANO | SHANO | BRMS rule will only allow 8 characters |
|  | SHASN | SHASN | BRMS rule will only allow 50 characters |
|  | LD1 | LD1 | This field is designated for address unit:  APT = Apartment  LOT = Lot  RM = Room  SLIP = Slip  SUIT = Suite  UNIT = Unit  Note: This is the format to be used on all forms for this field. |
|  | LD2 | LD2 | This field is designated for address elevation:  FLR – Floor  Note: This is the format to be used on all forms for this field. |
|  | LD3 | LD3 | This field is designated for address structure:  BLDG = Building  PIER = Pier  WNG = Wing  Note: This is the format to be used on all forms for this field. |
|  | ZIP | SHZIP | BRMS rule will only allow 5 characters |
| 3.3 Inside Wire |  |  |  |
|  | IWO | IWO | BRMS rule will not allow values of B, N, R, T, V or Y |
|  | IWBAN | IWBAN | For Information Only: CenturyLink does not have a current use for this information. If field data is populated by the customer, integrity edits are applied against field length, characteristics, and valid values. |
| 3.4 Bill Information |  |  |  |
|  | ZIP | ZIP | BRMS rule will only allow 5 characters |
| 3.5 Disconnect Information |  |  |  |
|  | DDD | N/A | Bulk requests DDD will use the LSR form DDD value |
|  | TERS | TERS | BRMS rule will only allow 4 characters |
|  | TC OPT | TC OPT | BRMS rule will only allow 1 character and not allow value of O |
|  | TC TO SEC | TC TO SEC | BRMS rule when TC OPT is T then TC TO SEC must be populated. |
| Loop Service Form (LS) | | | |
| 3.3 Service Details |  |  |  |
|  | LNUM | LNUM | BRMS rule to only allow 4 characters |
|  | Line Shared TN | SLTN | Use SLTN field for Line Sharing TN - 2Q19 allows 10 characters and IMA allowed 12 characters |
|  | CKR | CKR | BRMS rule to only allow 36 characters |
|  | ECCKT | ECCKT | 2Q19 allows 36 characters and IMA allowed 42 characters |
|  | CFA | CFA | 2Q19 allows 42 characters and IMA allowed 54 characters |
| 3.6 Transfer of Calls |  |  |  |
|  | DISC NBR | DISC NBR | 2Q19 allows 10 characters and IMA allowed 12  characters |
|  | TER | TERS | BRMS rule to only allow 8 characters |
|  | TC OPT | TC OPT | BRMS rule will only allow 1 character and not allow value of O |
|  | TC PER | TC PER | BRMS rule will only allow 8 characters |
|  | TC TO PRI | TC TO PRI | 2Q19 allows 10 characters and IMA allowed 12 characters |
|  | TC TO SEC | TC TO SEC | 2Q19 allows 10 characters and IMA allowed 12 characters. BRMS rule when TC OPT is T then TC TO SEC must be populated. |
| Remarks Section |  |  |  |
|  | REMARKS | REMARKS | 2Q19 allows 160 characters and IMA allowed 255 characters |
|  | MANUAL IND | N/A | Derived from LSR: NRI value of Y |
| Number Portability (NP) | | | |
| 3.3 Service Details |  |  |  |
|  | PORTED NBR | PORTED NBR | 2Q19 allows 15 characters and IMA allowed 17 characters |
|  | TC OPT | TC OPT | BRMS rule will only allow 1 character and not allow value of O |
|  | TC PER | TC PER | EASE Field in Service Details section– this field was in the Transfer of Calls Secondary Section in IMA |
|  | TC TO SEC | TC TO SEC | BRMS rule when TC OPT is T then TC TO SEC must be populated. |
| Loop Service with Number Portability (LSNP) | | | |
| 3.1 Administrative Section |  |  |  |
|  | LQTY | LQTY | BRMS rule will only allow 4 characters |
| 3.3 Service Details |  |  |  |
|  | LNUM | LNUM | BRMS rule to only allow 4 characters |
|  | CKR | CKR | BRMS rule to only allow 36 characters |
|  | ECCKT | ECCKT | 2Q19 allows 36 characters and IMA allowed 42 characters |
|  | CFA | CFA | 2Q19 allows 42 characters and IMA allowed 54 characters |
|  | PORTED NBR | PORTED NBR | BRMS rule to only allow 12 characters |
|  | CFTN | CFTN | BRMS rule to only allow 12 characters |
|  | BA | BA | IMA has value of E (end state) 2Q19 does not have E. Use value of A for end state |
|  | BLOCK | BLOCK | 2Q19 allows 16 characters and IMA had allowed 32 characters |
|  | REMARKS | REMARKS | 2Q19 allows 160 characters and IMA had allowed 255 characters |
|  | MANUAL IND | N/A | Derived from LSR: NRI value of Y |
| Resale Service (RS) | | | |
| 3.3 Service Details |  |  |  |
|  | LNUM | LNUM | BRMS rule to only allow 4 characters |
|  | NPI | NPI | Use value of E to indicate Port Within (IMA value was Z) |
|  | TNS | TNS | BRMS rule to only allow 12 characters |
|  | TERS | TERS | BRMS rule to only allow 4 characters |
|  | TLI | N/A | Use TLI field on Hunt Group Information form |
|  | OTN | OTN | 2Q19 allows 10 characters and IMA had allowed 12 characters |
|  | PRIDB | N/A | Data is provided on the IS form |
|  | ISPID | N/A | Data is provided on the IS form |
|  | PTLI | N/A | Data is provided in LTLI field on DDPS form |
|  | PTKCON | N/A | Data is provided in TTP field on DDPS form |
|  | MEGACENTNM | N/A | Will be set to default value of USWNET |
|  | SDI | N/A | Field on IS form |
|  | TC OPT | TC OPT | BRMS rule will only allow 1 character and not allow value of O |
|  | TC PER | TC PER | BRMS rule will only allow 8 character EASE Field in Service Details section– this field was in the Transfer of Calls Secondary Section in IMA |
| Transfer of Calls Secondary Section |  |  |  |
|  | TC TO SEC | TC TO SEC | BRMS rule when TC OPT is T then TC TO SEC must be populated. |
|  | BA | BA | IMA has value of E (end state) 2Q19 does not have E. Use value of A for end state |
|  | BLOCK | BLOCK | 2Q19 allows 16 characters and IMA had allowed 32 characters |
|  | CFA | CFA | 2Q19 allows 42 characters and IMA allowed 54 characters |
|  | FEATURE | FEATURE | BRMS rule to only allow 5 characters |
|  | FEATURE DETAIL | FEATURE DETAIL | 2Q19 allows 200 characters and IMA had allowed 512 characters |
|  | REMARKS | N/A | Derived from LSR Remarks |
|  | MANUAL IND | N/A | Derived from LSR: NRI value of Y |
| Resale Private Line (RPL) | | | |
| 3.2 Administrative Section |  |  |  |
|  | DQTY | DQTY | BRMS rule to only allow 3 characters |
| 3.3 Primary Location Section |  |  |  |
|  | NAME | N/A | Derive from NAME field on End User form |
|  | NCON | N/A | Derive from NCON field on End User form |
|  | AHN | AFT | When AHN is necessary, populate AFT with C (Provider assigned house number) and provide AHN numeric data in SANO field |
|  | SAPR | SAPR | BRMS rule will only allow 5 characters |
|  | SANO | SANO | BRMS rule will only allow 8 characters |
|  | SASN | SASN | BRMS rule will only allow 50 characters |
|  | LD1 | LD1 | This field is designated for address unit:  APT = Apartment  LOT = Lot  RM = Room  SLIP = Slip  SUIT = Suite  UNIT = Unit  Note: This is the format to be used on all forms for this field. |
|  | LD2 | LD2 | This field is designated for address elevation:  FLR – Floor  Note: This is the format to be used on all forms for this field. |
|  | LD3 | LD3 | This field is designated for address structure:  BLDG = Building  PIER = Pier  WNG = Wing  Note: This is the format to be used on all forms for this field. |
|  | AAI | AAI | 2Q19 field length 60 characters IMA was 100 characters |
|  | ZIP | ZIP | BRMS rule will only allow 5 characters |
|  | ACTEL NO | ACTEL NO | 2Q19 field length 14 characters IMA was 17 characters |
|  | AACTEL | AACTEL | 2Q19 field length 14 characters IMA was 17 characters |
|  | ACC | ACC | 2Q19 field length 45 and IMA was 255 |
| 3.4 Secondary Location Section |  |  |  |
|  | NCON | N/A | Derive from NCON field on End User form |
|  | AHN | AFT | When AHN is necessary, populate AFT with C (Provider assigned house number) and provide AHN numeric data in SANO field |
|  | SAPR | SAPR | BRMS rule will only allow 5 characters |
|  | SANO | SANO | BRMS rule will only allow 8 characters |
|  | SASN | SASN | BRMS rule will only allow 50 characters |
|  | LD1 | LD1 | This field is designated for address unit:  APT = Apartment  LOT = Lot  RM = Room  SLIP = Slip  SUIT = Suite  UNIT = Unit  Note: This is the format to be used on all forms for this field. |
|  | LD2 | LD2 | This field is designated for address elevation:  FLR – Floor  Note: This is the format to be used on all forms for this field. |
|  | LD3 | LD3 | This field is designated for address structure:  BLDG = Building  PIER = Pier  WNG = Wing  Note: This is the format to be used on all forms for this field. |
|  | AAI | AAI | 2Q19 field length 60 characters IMA was 100 characters |
|  | ZIP | ZIP | BRMS rule will only allow 5 characters |
|  | ACTEL NO | ACTEL NO | 2Q19 field length 14 characters IMA was 17 characters |
|  | AACTEL | AACTEL | 2Q19 field length 14 characters IMA was 17 characters |
|  | ACC | ACC | 2Q19 field length 45 and IMA was 255 |
| 3.5 Bill Section |  |  |  |
|  | FLOOR | FLOOR | 2Q19 field length 10 characters and IMA was 15 characters |
|  | ROOM/MAIL STOP | ROOM/MAIL STOP | 2Q19 field length 10 characters and IMA was 15 characters |
|  | ZIP | ZIP | BRMS rule will only allow 5 characters |
|  | TEL NO | TEL NO | 2Q19 field length 14 characters and IMA allowed 17 characters |
| 3.6 Disconnect Information |  |  |  |
|  | DISC ECCKT | DISC ECCKT | 2Q19 field length 36 characters and IMA allowed 42 characters |
| Remarks Section |  |  |  |
|  | REMARKS | REMARKS | 2Q19 field length 160 characters and IMA allowed 255 characters |
|  | MANUAL IND | N/A | Derived from LSR: NRI value of Y |
| 3.7 Primary Location Service Details |  |  |  |
|  | SAN | REMARKS | Enter SAN with value in the remarks (format SAN: then value) |
|  | ECCKT | ECCKT | 2Q19 field length 36 characters and IMA allowed 42 characters |
|  | CFA | CFA | 2Q19 field length 42 characters and IMA allowed 54 characters |
|  | FEATURE | FEATURE | BRMS rule will only allow 5 characters |
| 3.8 Secondary Location Service Details |  |  |  |
|  | CKR | CKR | 2Q19 field length 41 characters and IMA allowed 44 characters |
|  | ECCKT | ECCKT | 2Q19 field length 36 characters and IMA allowed 42 characters |
|  | CFA | CFA | 2Q19 field length 42 characters and IMA allowed 54 characters |
|  | FEATURE | FEATURE | BRMS rule will only allow 5 characters |
| Centrex Resale Services (CRS) | | | |
| 3.2 Administrative Section |  |  |  |
|  | RSQTY | RSQTY | BRMS rule will only allow 3 characters |
|  | ORD | ORD | BRMS rule will only allow 9 characters |
|  | CB | CB | 2Q19 field length 8 characters and IMA allowed 18 characters |
|  | CMS ID | CBFA | Set CBFA field to N along with CB\_FEATURE data of CMSID and CB\_FEATURE\_DETAILS populated with CMSID value |
| 3.3 Common Block Details |  |  |  |
|  | Not Used | CBFA | See notes below for use |
|  | Not Used | CB FEATURE | See notes below for use |
|  | Not Used | CB FEATURE DETAIL | See notes below for use |
|  | COS | CBFA CB FEATURE CB FEATURE DETAIL | Set CBFA field to N along with CB\_FEATURE data of COS and CB\_FEATURE\_DETAILS populated with COS value |
|  | XLI | CBFA CB FEATURE CB FEATURE DETAIL | Set CBFA field to N along with CB\_FEATURE data of XLI and CB\_FEATURE\_DETAILS populated with XLI value |
|  | DEPT | CBFA CB FEATURE CB FEATURE DETAIL | Set CBFA field to N along with CB\_FEATURE data of DEPT and CB\_FEATURE\_DETAILS populated with DEPT value |
|  | DPA | CBFA CB FEATURE CB FEATURE DETAIL | Set CBFA field to N along with CB\_FEATURE data of DPA and CB\_FEATURE\_DETAILS populated with DPA value |
|  | LOC | CBFA CB FEATURE CB FEATURE DETAIL | Set CBFA field to N along with CB\_FEATURE data of LOC and CB\_FEATURE\_DETAILS populated with LOC value |
|  | MIL | CBFA CB FEATURE CB FEATURE DETAIL | Set CBFA field to N along with CB\_FEATURE data of MIL and CB\_FEATURE\_DETAILS populated with MIL value |
| 3.4 Station Details |  |  |  |
|  | LNUM | LNUM | BRMS rule will only allow 4 characters |
|  | NPI | NPI | Use value of E to indicate Port Within (IMA value was Z) |
|  | TNS | TNS | BRMS rule will only allow 12 characters |
|  | TERS | TERS | BRMS rule will only allow 4 characters |
|  | TLI | N/A | Use TLI field on Hunt Group Information form |
|  | OTN | OTN | 2Q19 field length 10 characters and IMA allowed 12 characters |
|  | LTC | LTC | 2Q19 field length 2 characters and IMA allowed 3 characters |
|  | BA | BA | IMA has value of E (end state) 2Q19 does not have value of E. Use value of A for end state |
|  | BLOCK | BLOCK | 2Q19 allows 16 characters and IMA had allowed 32 characters |
|  | MEGACENTNM | N/A | Will be set to default value of USWNET |
|  | TC OPT | TC OPT | BRMS rule will only allow 1 character and not allow value of O |
|  | TC PER | TC PER | BRMS rule will only allow 8 characters EASE Field in Service Details section– this field was in the Transfer of Calls Secondary Section in IMA |
| Transfer of  Calls to Secondary Section |  |  |  |
|  | TC TO SEC | TC TO SEC | 2Q19 allows 10 characters and IMA allowed 12 characters – BRMS rule to required\ when TC OPT value is T |
|  | NIDR | N/A | If needed, add information in Remarks |
| Feature Information |  |  |  |
|  | FEATURE | FEATURE | BRMS rule will only allow 5 characters |
|  | FEATURE DETAIL | FEATURE DETAIL | 2Q19 field length 200 characters and IMA allowed 512 characters |
| Remarks Section |  |  |  |
|  | REMARKS | N/A | Derived from LSR Remarks |
|  | MANUAL IND | N/A | Derived from LSR: NRI value of Y |
| DID/DOD/PBX Service (DDPS) – Compared to IMA Resale form (RS) | | | |
| 3.3 Common Section |  |  |  |
|  | LNUM | RNUM | Use RNUM field |
|  | NPI | NPI | Use value of E to indicate Port Within (IMA value was Z) |
| 3.4 DID/DOD Telephone Number Section |  |  |  |
|  | LNUM | RNUM | Use RNUM field |
|  | LNA | TNA | Use TNA field |
|  | TNS | TNS | BRMS rule to only allow 12 characters. Also no range of TNs allowed |
|  | OTN | OTNS | BRMS rule to only allow 12 characters. Also no range of TNs allowed |
|  | ECCKT | ECCKT | 2Q19 allows 36 characters and IMA had allowed 42 characters |
| 3.5 Trunk Service Detail |  |  |  |
|  | LNA | TACT | Use TACT field |
|  | TERS | TERS | BRMS rule to only allow 4 characters. |
|  | TNS | TNS | BRMS rule to only allow 12 characters. Also no range of TNs allowed |
|  | OTN | OTN | BRMS rule to only allow 12 characters. Also no range of TNs allowed |
|  | TLI | LTLI | Use LTLI field. 2Q19 allows 10 characters and IMA had allowed 12 characters |
|  | ECCKT | ECCKT | 2Q19 allows 36 characters and IMA had allowed 42 characters |
|  | BA | BA | IMA has value of E (end state) 2Q19 does not have value of E. Use value of A for end state |
|  | BLOCK | BLOCK | 2Q19 allows 16 characters and IMA had allowed 32 characters |
|  | MEGACENTNM | N/A | Not needed for product |
| 3.6 Feature Section |  |  |  |
|  | LNUM | RNUM | Use RNUM field |
|  | FEATURE | FEATURE | BRMS rule will only allow 5 characters |
|  | FEATURE DETAIL | FEATURE DETAIL | 2Q19 field length 200 characters and IMA allowed 512 characters |
| 3.7 Transfer of Calls Details |  |  |  |
|  | LNUM | RNUM | Use RNUM field |
|  | TC OPT | TC OPT | BRMS rule will only allow 1 character and not allow value of O |
|  | TC PER | TC PER | BRMS rule will only allow 8 character |
|  | TC TO SEC | TC TO SEC | BRMS rule when TC OPT is T then TC TO SEC must be populated. |
|  | REMARKS | REMARKS | 2Q19 allows 160 characters and IMA allowed 255 characters |
|  | MANUAL IND | N/A | Derived from LSR: NRI value of Y |
| DID/DOD/PBX Service (DDPS) – Compared to IMA DID Resale form (DRS) | | | |
| 3.3 Common Section |  |  |  |
|  | DIDNUM | RNUM | BRMS rule to only allow 3 characters |
|  | NPI | NPI | Use value of E to indicate Port Within (IMA value was Z) |
| 3.4 DID/DOD Telephone Number Section |  |  |  |
|  | DIDNUM | RNUM | BRMS rule to only allow 3 characters |
|  | DTNRACT | TNA | Use TNA field |
|  | DTNRQ | QN | Use QN field |
|  | CKR | CKR | 2Q19 field length 41 characters and IMA allowed 44 characters |
|  | DTNR | TNS | Use TNS field |
|  | DSTNACT | DA | Use DA field |
|  | DTGN | TGN | Use TGN field |
|  | DRTI | RIN | BRMS rule to only allow 4 characters |
| 3.5 Trunk Service Detail Section |  |  |  |
|  | DIDNUM | RNUM | BRMS rule to only allow 3 characters |
|  | DTKACT | TACT | Use TACT field |
|  | DTK | TKQ | Use TKQ field |
|  | DTNR | TNS | BRMS rule to only allow 12 characters. Also no range of TNs allowed |
|  | DTLI | LTLI | Use LTLI field |
|  | DTGN | TGN | Use TGN field |
|  | DRTI | RIN | BRMS rule to only allow 4 characters |
|  | DTKID | TKID | Use TKID field |
|  | DGOUT | DO | Use DO field |
|  | DPULSE | PULSE | Use PULSE field |
|  | DSGNL | SGNL | Use SGNL field |
| 3.6 Feature Section |  |  |  |
|  | DIDNUM | RNUM | BRMS rule to only allow 3 characters |
|  | FEATURE | FEATURE | BRMS rule will only allow 5 characters |
|  | FEATURE DETAIL | FEATURE DETAIL | 2Q19 field length 200 characters and IMA allowed 512 characters |
| 3.7 Transfer of Calls Details |  |  |  |
|  | LNUM | RNUM | Use RNUM field |
|  | TC OPT | TC OPT | BRMS rule will only allow 1 character and not allow value of O |
|  | TC PER | TC PER | BRMS rule will only allow 8 character |
|  | TC TO SEC | TC TO SEC | BRMS rule when TC OPT is T then TC TO SEC must be populated. |
|  | REMARKS | REMARKS | 2Q19 allows 160 characters and IMA allowed 255 characters |
|  | MANUAL IND | N/A | Derived from LSR: NRI value of Y |
| Hunt Group Information (HGI) | | | |
| 3. Hunt Group |  |  |  |
|  | HID | HID | BRMS rule to only allow 5 characters. BRMS rule to not allow value of N |
|  | TLI | TLI | BRMS rule to only allow 10 characters. |
| 3.3 Hunt Detail Section |  |  |  |
|  | HTSEQ | HTSEQ | 2Q19 field length 10 characters and IMA was 512 characters.  Example how to use HTSEQ and HTN fields: HTSEQ A HTN 303-555-0001  HTSEQ A HTN 303-555-0002  HTSEQ B HTN 303-555-0003  HTSEQ B HTN 303-555-0004 |
| ISDN BRI/PRI Service (IS) – Compared to IMA Resale form (RS) | | | |
| 3.2 Service Details |  |  |  |
|  | LNUM | LNUM | BRMS rule to only allow 4 characters |
|  | NPI | NPI | Use value of E to indicate Port Within (IMA value was Z) |
|  | TNS | TNS | BRMS rule to only allow 12 characters. Also no range of TNs allowed |
|  | OTN | OTN | 2Q19 allows 10 characters and IMA allowed 12 characters |
|  | TERS | TERS | BRMS rule to only allow 4 characters |
|  | ECCKT | ECCKT | 2Q19 allows 36 characters and IMA allowed 42 characters |
|  | MEGACENTNM | N/A | Will be set to default value of USWNET |
|  | TC OPT | TC OPT | BRMS rule will only allow 1 character and not allow value of O |
|  | TC PER | TC PER | BRMS rule will only allow 8 character |
|  | TC TO SEC | TC TO SEC | BRMS rule when TC OPT is T then TC TO SEC must be populated. |
|  | ISPID | ISPID | 2Q19 allows 14 characters and IMA allowed 15 characters (don’t add dash in EASE) |
|  | BA | BA | IMA has value of E (end state) 2Q19 does not have E. Use value of A for end state |
|  | BLOCK | BLOCK | 2Q19 allows 16 characters and IMA had allowed 32 characters |
|  | CFA | CFA | 2Q19 allows 42 characters and IMA allowed 54 characters |
|  | FEATURE | FEATURE | BRMS rule will only allow 5 characters |
|  | FEATURE DETAIL | FEATURE DETAIL | 2Q19 field length 200 characters and IMA allowed 512 characters |
| Remarks Section |  |  |  |
|  | REMARKS | N/A | Derived from LSR: Remarks |
|  | MANUAL IND | N/A | Derived from LSR: NRI value of Y |
| Directory Listing (DL) | | | |
|  | FBDL CCNA | LSR form OCCNA field | Associated with LNP and the data will be obtained from LSR form OCCNA field |
|  | FBDL CC |  | Associated with LNP and the data will be obtained from LSR form OCC field |
| 4.2 Listing Control Section |  |  |  |
|  | DDQTY | N/A | Derived by CenturyLink |
| 4.4 Listing Instruction |  |  |  |
|  | LTEXT | LTEXT | BRMS rule to only allow 100 characters |
|  | LAPR | LAPR | BRMS rule to only allow 5 characters |
|  | LANO | LANO | BRMS rule to only allow 8 characters |
|  | LASN | LASN | BRMS rule to only allow 50 characters |
| 4.6 Deliver Address/ Information Section |  |  |  |
|  | NAME | NAME | BRMS rule to only allow 25 characters |
|  | DDAPR | DDAPR | BRMS rule to only allow 5 characters |
|  | DDANO | DDANO | BRMS rule to only allow 8 characters |
|  | DDASN | DDASN | BRMS rule to only allow 50 characters |
|  | LD1 | LD1 | This field is designated for address unit: APT = Apartment LOT = Lot RM = Room SLIP = Slip SUIT = Suite UNIT = Unit Note: This is the format to be used on all forms for this field. |
|  | LD2 | LD2 | This field is designated for address elevation:  FLR – Floor  Note: This is the format to be used on all forms for this field. |
|  | LD3 | LD3 | This field is designated for address structure:  BLDG = Building  PIER = Pier  WNG = Wing  Note: This is the format to be used on all forms for this field. |
|  | AAI | AAI | BRMS rule to only allow 30 characters |
|  | ZIP | ZIP | BRMS rule will only allow 5 characters |
|  | REMARKS | REMARKS | 2Q19 field length 160 characters and IMA was 255 characters |
| Miscellaneous | | | |
| CLSP POTS SPLIT, CLSP Centrex SPLIT or CLSP PBX SPLIT LSRs (Line Splitting products) | REQTYP and TOS | POTSSPLITLOC | Will be identified by EASE when the POTSSPLITLOC field is populated |